Power Supply Chassis

Phonoclone Chassis

Power Supply Case

XLR Plug

3-pin female

16 AWG 3-conductor unshielded power cord

1A 200V

35 VA Transformer

12 VAC

12 VAC

V++ to XLR pin 1

V-- to XLR pin 2

COM to XLR pin 3

Earth

(not connect ed to COM)

Neutral

Live

0.5A SB fuse

Connect

screen to case

Pin 1

Pin 3

Pin 2

RCA

Output L

RCA

Output R

RCA

Input R

RCA

Input L

Phonoclone 3 PCB

Phonoclone 3 PCB

Ground Lug

and Case

XLR Jack

3-pin male

IN+

IN-

OUT+

OUT-

V-- COM V++

IN+

IN-

OUT+

OUT-

V-- COM V++